[General]
adviseFail=15
adviseObsRate=
adviseReco=5
adviseScript=
autoStart=0
casterUrlList=http://Example:Configs@products.igs-ip.net:2101, http://bkg:realtime06@igs-ip.net:2101, http://bkg:realtime06@euref-ip.net:2101
cmbBds=2
cmbBsxFile=
cmbGal=2
cmbGlo=2
cmbGps=2
cmbLogpath=
cmbMaxdisplacement=
cmbMaxres=
cmbMethod=Kalman Filter
cmbNavic=0
cmbQzss=0
cmbSampl=1 sec
cmbSbas=0
cmbStreams=
corrIntr=1 day
corrPath=
corrPort=
ephIntr=1 day
ephOutPort=
ephPath=
ephVersion=4
font=
logFile=Output/PPP.log
miscIntr=
miscMount=
miscPort=
miscScanRTCM=0
mountPoints=//Example:Configs@euref-ip.net:2101/WTZR00DEU0 RTCM_3.3 DEU 49.14 12.88 no 2, //Example:Configs@products.igs-ip.net:2101/BCEP00BKG0 RTCM_3.3 DEU 50.09 8.66 no 2, //Example:Configs@products.igs-ip.net:2101/SSRA00CNE1 RTCM_3.1 FRA 43.56 1.48 no 2
ntripVersion=2
onTheFlyInterval=no
outFile=
outLockTime=0
outPort=
outSampl=1 sec
outUPort=
outWait=1
proxyHost=
proxyPort=
rawOutFile=Output/raw.rtcm
reqcAction=
reqcComment=
reqcEndDateTime=2099-01-01T00:00:00
reqcLogSummaryOnly=0
reqcNavFile=
reqcNewAntennaName=
reqcNewAntennaNumber=
reqcNewAntennadE=
reqcNewAntennadN=
reqcNewAntennadU=
reqcNewMarkerName=
reqcNewReceiverName=
reqcNewReceiverNumber=
reqcObsFile=
reqcOldAntennaName=
reqcOldAntennaNumber=
reqcOldAntennadE=
reqcOldAntennadN=
reqcOldAntennadU=
reqcOldMarkerName=
reqcOldReceiverName=
reqcOldReceiverNumber=
reqcOutLogFile=
reqcOutNavFile=
reqcOutObsFile=
reqcPlotDir=
reqcRnxVersion=
reqcRunBy=
reqcSampling=1 sec
reqcSkyPlotSignals=G:1&2&5 R:1&2&3 E:1&7 C:2&6 J:1&2 I:5&9 S:1&5
reqcStartDateTime=1967-11-02T00:00:00
reqcUseObsTypes=
reqcV2Priority=G:12&PWCSLX G:5&IQX R:12&PC R:3&IQX R:46&ABX E:16&BCXZ E:578&IQX J:1&SLXCZ J:26&SLX J:5&IQX C:267&IQX C:18&DPX I:ABCX S:1&C S:5&IQX
rnxAppend=0
rnxIntr=1 day
rnxOnlyWithSKL=0
rnxPath=
rnxSampl=1 sec
rnxScript=
rnxSkel=skl
rnxSkelPath=
rnxV2Priority=G:12&PWCSLX G:5&IQX R:12&PC R:3&IQX R:46&ABX E:16&BCXZ E:578&IQX J:1&SLXCZ J:26&SLX J:5&IQX C:267&IQX C:18&DPX I:ABCX S:1&C S:5&IQX
rnxVersion=4
serialAutoNMEA=Auto
serialBaudRate=9600
serialDataBits=8
serialFileNMEA=
serialFlowControl=OFF
serialHeightNMEA=
serialManualNMEASampling=10
serialMountPoint=
serialNMEASampling=0
serialParity=NONE
serialPortName=
serialStopBits=1
sp3CompExclude=
sp3CompFile=
sp3CompOutLogFile=
sp3CompSummaryOnly=0
sslCaCertPath=
sslClientCertPath=
sslIgnoreErrors=0
startTab=12
statusTab=3
trafo_dx=
trafo_dxr=
trafo_dy=
trafo_dyr=
trafo_dz=
trafo_dzr=
trafo_ox=
trafo_oxr=
trafo_oy=
trafo_oyr=
trafo_oz=
trafo_ozr=
trafo_sc=
trafo_scr=
trafo_t0=
uploadAntexFile=
uploadEphMountpointsOut=
uploadIntr=1 day
uploadMountpointsOut=
uploadRawMountpointsOut=
uploadSamplBiaSnx=5
uploadSamplClkRnx=0
uploadSamplRtcmEph=5
uploadSamplRtcmEphCorr=5 sec
uploadSamplSp3=30 sec

[PPP]
antexFile=Input/igs20.atx
arBDS=0
arGPS=2
arGalileo=2
arMaxFrac=0.01
arMaxSig=0.001
arMinEle=10
arMinNumEpo=30
arMinNumSat=5
arUseYaw=0
audioResponse=
biasFile=
biasMount=
blqFile=Input/BNC.BLQ
constraints=no
corrFile=
corrMount=SSRA00CNE1
corrWaitTime=5
crdFile=Input/BNC_IGS20.CRD
dataSource=Real-Time Streams
eleWgtCode=2
eleWgtPhase=2
ionoFile=
ionoMount=
lcBDS=P26&L26
lcGLONASS=Pi&Li
lcGPS=P12&L125
lcGalileo=P15&L1576
logMode=normal
logPath=Output
mapSpeedSlider=100
mapWinDotColor=red
mapWinDotSize=6
maxResC1=3.0
maxResGIM=5.0
maxResL1=0.03
minEle=10
minObs=5
modelObs=Uncombined PPP
nmeaPath=
plotCoordinates=WTZR00DEU0
pseudoObs=no
rinexNav=
rinexObs=
seedingTime=0
sigmaC1=1.0
sigmaGIM=5.0
sigmaL1=0.02
snxtroAc=
snxtroCampId=
snxtroIntr=1 hour
snxtroPath=
snxtroSampl=1 sec
snxtroSolId=
snxtroSolType=
staTable="WTZR00DEU0,100.0,100.0,100.0,100.0,100.0,100.0,0.1,3e-6,0,G:1&C G:2&W G5:I E:16&C E:57&Q C:26&I,"
